GSIC - Global Service Information Center

# 1GR-FE FUEL > SERVICE DATA

Fuel pressure | 281 to 287 kPa (2.87 to 2.93 kgf/cm2, 40.8 to 41.7 psi
Fuel pressure | 147 kPa (1.5 kgf/cm2, 21 psi) or more
Fuel injector | Resistance | at 20°C (68°F) | 11 to 12.4 Ω
Injection volume | 76 to 91 cm3 (4.6 to 5.5 cu in.) per 15 seconds
Difference between each cylinder | 15 cm3 (0.9 cu in.) or less
Fuel leakage | 1 drop or less per 12 minutes
Fuel pump resister | Resistance | at 20°C (68°F) | 0.70 to 0.76 Ω
Fuel pump | Resistance | at 20°C (68°F) | 0.2 to 3.0 Ω
Fuel pump relay assembly | Specified condition | 3 - 4 | Below 1 Ω
3 - 5 | 10 kΩ or higher
3 - 5 | Below 1 Ω