GSIC - Global Service Information Center

# POWER DOOR LOCK CONTROL SYSTEM > ON-VEHICLE INSPECTION

1. CHECK POWER DOOR LOCK OPERATION

1. Check the basic function.

   1. Check that all doors lock when the door control switch (for manual operation) LOCK side is pressed, and that all doors unlock when the UNLOCK side is pressed.

   2. Check that all doors lock when the driver side door lock key cylinder is turned to LOCK using the key. However, the driver side door key-linked lock and unlock function will not operate when the seat belt is fastened.