GSIC - Global Service Information Center

# HEADLIGHT DIMMER SWITCH > INSTALLATION

## for Preparation Click here

1. INSTALL HEADLIGHT DIMMER SWITCH ASSEMBLY

1. Install the headlight dimmer switch with the claw as shown in the illustration.

1. Install the headlight dimmer switch with the clamp.

1. Connect the connector.

2. INSTALL WIPER AND WASHER SWITCH ASSEMBLY

1. Attach the claw to install the wiper switch.

1. Connect the connectors.

   NOTICE:
     Do not push the claw with excessive force as damage may occur.

3. INSTALL SPIRAL CABLE SUB-ASSEMBLY

1. Check that the front wheels are facing straight ahead.

1. Set the turn signal switch to the neutral position.

   NOTICE:
     Make sure that the turn signal switch is in the neutral position, as the pin of the turn signal switch may be snapped.

1. Install the spiral cable.

   NOTICE:
     When replacing the spiral cable with a new one, remove the lock pin before installing the steering wheel.

1. Connect the connectors to the spiral cable.

   NOTICE:
     When handling the airbag connector, do not damage the airbag wire harness.

4. INSTALL STEERING COLUMN COVER UPPER

1. Install the cover lower with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

5. INSTALL STEERING COLUMN COVER LOWER

1. Install the cover lower with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

6. INSTALL STEERING WHEEL ASSEMBLY

1. Align the matchmarks on the steering wheel and main shaft.

1. Install the steering set nut.

   Torque:
     50 N*m{ 510 kgf*cm , 37 ft.*lbf }

7. PLACE FRONT WHEELS FACING STRAIGHT AHEAD

8. INSPECT STEERING WHEEL CENTER POINT

9. INSTALL STEERING PAD ASSEMBLY

1. Support the steering pad with one hand as shown in the illustration.

1. Connect the airbag connector.

   NOTICE:
     When handling the airbag connector, do not damage the airbag wire harness.

1. Connect the horn connector.

1. Install the steering pad after confirming that the circumference grooves of the screws are caught on the screw case.

1. Using a T30 "torx" socket, install the 2 screws.

   Torque:
     8.8 N*m{ 90 kgf*cm , 78 in.*lbf }

10. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

11. INSPECT STEERING PAD ASSEMBLY

1. Check for cuts, cracks or discoloration on the steering pad outer surface and in the grooved portion.

1. Check that the horn sounds.

12. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

13. CHECK SRS WARNING LIGHT

1. Check the SRS warning light (Click here).