GSIC - Global Service Information Center

# BRAKE > SERVICE DATA

Brake pedal height from dash panel | LHD (M/T) | 152.9 to 162.9 mm (6.020 to 6413 in.)
LHD (A/T) | 154.1 to 1164.1 mm (6.067 to 6.461 in.)
RHD (M/T) | 156.9 to 166.9 mm (6.177 to 6.571 in.)
RHD (A/T) | 158.1 to 168.1 mm (6.224 to 6.618 in.)
Brake pedal free play Stop light switch clearance | 1.0 to 6.0 mm (0.039 to 0.236 in.)
1.5 to 2.5 mm (0.059 to 0.098 in.)
Brake pedal reserve distance from dash panel | LHD (2WD) | 78.0 mm (3.071 in.)
LHD (4WD) | 85.0 mm (3.347 in.)
RHD (2WD) | 82.0 mm (3.228 in.)
RHD (4WD) | 89.0 mm (3.504 in.)
Booster push rod and accessory tool clearance Negative pressure of vacuum pump assembly | 0 mm (0 in.)
More than 86.7 kPa (650 mmHg, 26 in.Hg)
Front pad lining thickness (2WD) | Standard | 10.0 mm (0.394 in.)
Minimum | 1.0 mm (0.039 in.)
Front disc thickness (2WD) | Standard | 28.0 mm (1.102 in.)
Minimum | 26.0 mm (1.024 in.)
Front disc runout (2WD) | Maximum | 0.05 mm (0.0020 in.)
Front pad lining thickness (4WD) | Standard | 11.5 mm (0.453 in.)
Minimum | 1.0 mm (0.039 in.)
Front disc thickness (4WD) | Standard | 25.0 mm (0.984 in.)
Minimum | 23.0 mm (0.906 in.)
Front disc runout (4WD) | Maximum | 0.05 mm (0.0020 in.)
Rear brake drum inside diameter (2WD) | Standard | 254.0 mm (10.000 in.)
Maximum | 256.0 mm (10.079 in.)
Rear brake shoe lining thickness (2WD) | Standard | 5.1 mm (0.201 in.)
Minimum | 1.0 mm (0.039 in.)
Rear brake drum and rear brake shoe clearance (2WD) | 0.5 mm (0.020 in.)
Rear brake drum inside diameter (4WD) | Standard | 295.0 mm (11.614 in.)
Maximum | 297.0 mm (11.693 in.)
Rear brake shoe lining thickness (4WD) | Standard | 5.4 mm (0.213 in.)
Minimum | 1.0 mm (0.039 in.)
Rear brake drum and rear brake shoe clearance (4WD) | 0.6 mm (0.024 in.)