GSIC - Global Service Information Center

# PARK / NEUTRAL POSITION SWITCH > ADJUSTMENT

## for Preparation Click here

1. ADJUST PARK/NEUTRAL POSITION SWITCH ASSEMBLY

1. Loosen the park/neutral position switch bolt and move the shift lever to N.

1. Align the switch groove with the neutral basic line.

1. Hold the switch in position and tighten the bolt.

   Torque:
     13 N*m{ 130 kgf*cm , 9 ft.*lbf }

1. After adjustment, perform the inspection (Click here).