GSIC - Global Service Information Center

# CONDENSER (for 2KD-FTV) > ON-VEHICLE INSPECTION

## for Preparation Click here

1. CHECK COOLER CONDENSER ASSEMBLY

1. If the fins of the cooler condenser are dirty, clean them with water. Dry the fins with compressed air.

   NOTICE:
     Do not damage the fins of the condenser.

1. If a fin of the cooler condenser is bent, straighten it using a screwdriver or pliers.

2. CHECK CONDENSER FOR LEAKAGE OF REFRIGERANT

1. Using a halogen leak detector, check the pipe joints for gas leakage.

1. If gas leakage is detected in a joint, check the torque of the joint.