GSIC - Global Service Information Center

# IGNITION COIL > INSTALLATION

## for Preparation Click here

1. INSTALL IGNITION COIL ASSEMBLY

1. Install the ignition coil with the bolt.

   Torque:
     9.0 N*m{ 92 kgf*cm , 80 in.*lbf }

1. Connect the connector.

2. INSTALL AIR CLEANER ASSEMBLY

Torque:
  8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

3. INSTALL V-BANK COVER

Torque:
  7.5 N*m{ 76 kgf*cm , 66 in.*lbf }

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting the cable from the negative (-) battery terminal.