GSIC - Global Service Information Center

# FRONT DOOR COURTESY SWITCH > INSPECTION

## for Preparation Click here

1. INSPECT FRONT DOOR COURTESY LIGHT SWITCH ASSEMBLY

1. Measure the resistance of the switch.

   Standard resistance:
   Tester Connection | Switch Condition | Specified Condition
   1 - Switch body | Pushed | 10 kΩ or higher
   1 - Switch body | Not pushed | Below 1 Ω

   If the result is not as specified, replace the switch assembly.