GSIC - Global Service Information Center

# REAR SEAT ASSEMBLY (for Extra Cab) > DISASSEMBLY

## for Preparation Click here

1. REMOVE REAR SEAT CUSHION COVER LH

1. Remove the 14 hog rings and the seat cushion cover from the seat cushion pad.

2. REMOVE REAR SEAT CUSHION COVER RH

HINT:

  Use the same procedures described for the LH side.

3. REMOVE REAR SEATBACK COVER

1. Remove the 20 hog rings and the seatback cover from the seatback pad.