GSIC - Global Service Information Center

# LICENSE PLATE LIGHT ASSEMBLY > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE LICENSE PLATE LIGHT ASSEMBLY

1. Detach the 2 claws and remove the license plate light.

1. Disconnect the connector.

3. REMOVE LICENSE PLATE LIGHT BULB

1. Turn the bulb/socket unit in the direction indicated by the arrow and pull to remove it.

1. Remove the bulb from the socket.