GSIC - Global Service Information Center

# FRONT SEAT ASSEMBLY (for Bench Seat Type) > REASSEMBLY

## for Preparation Click here

CAUTION:

  Wear protective gloves. Sharp areas on the seatback spring and seat cushion frame may injure your hands.

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the RH side.

1. INSTALL FRONT SEAT CUSHION COVER

NOTICE:

1. Be careful not to damage the cover.
2. When installing the hog rings, avoid wrinkling the cover.

1. Using hog ring pliers, install the seat cushion cover to the seat cushion pad with 6 new hog rings.

1. Using hog ring pliers, install the seat cushion cover (with pad) to the seat cushion frame with 18 new hog rings.

1. w/ Occupant detection sensor:
   Attach the sensor clamp.

2. INSTALL FRONT SEATBACK COVER

NOTICE:

1. Be careful not to damage the cover.
2. When installing the hog rings, avoid wrinkling the cover.

1. Using hog ring pliers, install the seatback cover to the seatback pad with 2 new hog rings.

1. Install the seatback cover (with pad) to the seatback frame.

1. Attach the 4 claws to install the 2 headrest supports.

1. Using hog ring pliers, install 5 new hog rings.

1. Close the fastening tapes.

3. INSTALL FRONT SEATBACK ASSEMBLY

1. Install the seatback with the 4 bolts.

   Torque:
     40 N*m{ 408 kgf*cm , 30 ft.*lbf }

4. INSTALL FRONT SEAT CUSHION SHIELD INNER RH

1. Attach the 2 claws and install the cushion shield with the screw.

5. INSTALL FRONT SEAT CUSHION SHIELD RH

HINT:

  Use the same procedures described for the cushion shield inner RH.

6. INSTALL RECLINING ADJUSTER RELEASE HANDLE RH

1. Install the release handle with the screw.