GSIC - Global Service Information Center

# FRONT DOOR BELT MOULDING > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT DOOR WINDOW REGULATOR HANDLE ASSEMBLY (w/o Power Window)

3. REMOVE FRONT DOOR LOWER FRAME BRACKET GARNISH LH

4. REMOVE DOOR PULL HANDLE

5. REMOVE FRONT ARMREST BASE PANEL UPPER LH (w/ Power Window)

6. REMOVE FRONT DOOR TRIM BOARD SUB-ASSEMBLY LH

7. REMOVE OUTER REAR VIEW MIRROR SUB-ASSEMBLY LH

8. REMOVE FRONT DOOR BELT MOULDING ASSEMBLY LH

1. Put protective tape under the moulding.

1. Using a moulding remover, pry out the moulding as shown in the illustration.

   HINT:
     Tape the remover tip before use.

   NOTICE:
     Be careful when removing the moulding as there are claws attached to the moulding.