GSIC - Global Service Information Center

# REAR BUMPER (for Flat Type) > DISASSEMBLY

## for Preparation Click here

1. REMOVE LICENSE PLATE LIGHT ASSEMBLY

1. Detach the 4 claws and remove 2 lights.

2. REMOVE REAR BUMPER PLATE

1. Using a screwdriver, detach the 13 claws and remove the bumper plate.

   HINT:
     Tape the screwdriver tip before use.

3. REMOVE REAR BUMPER PLATE LH

1. Using a screwdriver, detach the 2 claws and remove the plate.

   HINT:
     Tape the screwdriver tip before use.

4. REMOVE REAR BUMPER PLATE RH

HINT:

  Use the same procedures described for the LH side.

5. REMOVE REAR BUMPER BAR PLATE

1. Using a heat light, heat the bumper bar plate.

   Standard:

     Item | Heating Temperature
     Rear bumper bar plate | 20 to 30°C (68 to 86°F)

   NOTICE:
     Do not heat the bumper bar plate excessively.

1. Pull off the bumper bar plate by cutting the double-sided tape with a knife.

   NOTICE:
     Be careful not to damage the bumper bar.

1. Using a screwdriver, detach the 12 claws and remove the bumper bar plate from the bumper bar.

   HINT:
     Tape the screwdriver tip before use.