GSIC - Global Service Information Center

### COMPRESSOR AND PULLEY (for 2KD-FTV) > INSTALLATION

1. ADJUST COMPRESSOR OIL

2. INSTALL COOLER COMPRESSOR ASSEMBLY

3. INSTALL NO. 1 COOLER REFRIGERANT DISCHARGE HOSE

4. INSTALL SUCTION HOSE SUB-ASSEMBLY

5. INSTALL DRIVE BELT

6. INSTALL AIR CLEANER ASSEMBLY

7. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

8. PERFORM INITIALIZATION

9. CHARGE REFRIGERANT

10. WARM UP ENGINE

11. CHECK FOR LEAKAGE OF REFRIGERANT