GSIC - Global Service Information Center

# 2TR-FE LUBRICATION > SERVICE DATA

Oil pressure : at idle | 29 kPa (0.3 kgf/cm2, 4.2 psi) or more
Oil pressure : at 3,000 rpm | 160 to 490 kPa (1.6 to 5.0 kgf/cm2, 4.2 to 71 psi) or more
Oil pump : Tip clearance | Standard: 0.040 to 0.160 mm (0.0016 to 0.0063 in.) Maximum: 0.26 mm (0.0102 in.)
Oil pump : Side clearance | Standard: 0.025 to 0.075 mm (0.0010 to 0.0030 in.) Maximum: 0.130 mm (0.0051 in.)
Oil pump : Body clearance | Standard: 0.025 to 0.325 mm (0.0010 to 0.0128 in.) Maximum: 0.425 mm (0.0167 in.)