GSIC - Global Service Information Center

# CIGARETTE LIGHTER > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE SWITCH BASE

1. Detach the 8 claws.

1. Disconnect all connectors and remove the switch base.

3. REMOVE CIGARETTE LIGHTER COVER

1. Detach the 2 claws and remove the cover.

4. REMOVE CIGARETTE LIGHTER ASSEMBLY

1. Rotate the cigarette lighter socket to disengage the cigarette lighter bezel stay's notch from the socket hole.

   NOTICE:
     Do not damage the bulb terminal.

1. Pull out the socket halfway.

1. Align the socket with the stay's grooves and remove the socket.