GSIC - Global Service Information Center

# REAR SEAT ASSEMBLY (for Extra Cab) > INSTALLATION

## for Preparation Click here

1. INSTALL REAR SEATBACK ASSEMBLY

1. Place the seat in the cabin.

   NOTICE:
     Be careful not to damage the vehicle body.

1. Attach the seatback's 2 hooks to the vehicle body.

1. Install the seat with the 2 bolts.

   Torque:
     39 N*m{ 398 kgf*cm , 29 in.*lbf }

2. INSTALL BACK PANEL GARNISH LOWER

1. Attach the 5 clips and 6 claws to install the garnish.

3. INSTALL BACK PANEL GARNISH UPPER

1. Attach the 5 clips and 4 claws to install the garnish.

4. INSTALL REAR SEAT CUSHION ASSEMBLY LH

1. Attach the seat cushion's 2 rear hooks to the vehicle body.

1. Attach the seat cushion's front hook to the rear seat cushion lock hook. Then install the seat cushion.

1. Confirm that the seat cushion is firmly installed.

5. INSTALL REAR SEAT CUSHION ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.