GSIC - Global Service Information Center

# FRONT PASSENGER AIRBAG ASSEMBLY > REMOVAL

## for Preparation Click here

CAUTION:

  Be sure to read the precautionary notices concerning the SRS airbag system before servicing (Click here).

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE GLOVE COMPARTMENT DOOR ASSEMBLY

1. Push in the sides of the glove compartment door, as indicated by the arrows in the illustration. Then open the door to release it from the 2 stoppers. Open the door until it is horizontal.

1. Pull the glove compartment door toward the rear of the vehicle to detach the 2 hinges and remove the glove compartment door.

3. REMOVE FRONT PASSENGER AIRBAG ASSEMBLY

1. Disconnect the connector from the airbag.

   NOTICE:
     When handling the airbag connector, do not damage the airbag wire harness.

1. Remove the 2 bolts.

1. Detach the clamp from the bracket.

1. Detach the 12 claws and remove the airbag.