GSIC - Global Service Information Center

# SUN GEAR AND ONE-WAY CLUTCH > INSPECTION

## for Preparation Click here

1. INSPECT ONE-WAY CLUTCH ASSEMBLY

1. Hold the planetary sun gear, and turn the one-way clutch assembly. Check that the one-way clutch hub can be turned freely clockwise and locks when turned counterclockwise.

2. INSPECT PLANETARY SUN GEAR

1. Using a dial indicator, measure the inside diameter of the planetary sun gear bushes.

   Maximum inside diameter:
     27.08 mm (1.0661 in.)
   If the inside diameter is greater than the maximum, replace the planetary sun gear.