GSIC - Global Service Information Center

### WIRELESS DOOR LOCK CONTROL SYSTEM > Only Wireless Control Function is Inoperative

DESCRIPTION

WIRING DIAGRAM

INSPECTION PROCEDURE

CHECK WIRELESS DOOR LOCK CONTROL FUNCTIONS

CHECK THAT TRANSMITTER LED ILLUMINATES

CHECK WIRELESS DOOR LOCK CONTROL FUNCTION (STANDARD OPERATION FUNCTION)

REPLACE TRANSMITTER BATTERY

CHECK NO.1 ROOM LIGHT ASSEMBLY

SWITCH TO SELF-DIAGNOSTIC MODE

CHECK BY SELF-DIAGNOSTIC MODE

REGISTER RECOGNITION CODE

CHECK RESPONSE OF DOOR CONTROL RECEIVER

REPLACE DOOR CONTROL RECEIVER

CONFIRM INPUT METHOD OF SELF-DIAGNOSTIC MODE

INSPECT UNLOCK WARNING SWITCH ASSEMBLY

CHECK WIRE HARNESS (DOOR CONTROL RECEIVER - INSTRUMENT PANEL JUNCTION BLOCK)

CHECK DOOR CONTROL RECEIVER (OUTPUT)

REPLACE DOOR CONTROL TRANSMITTER MODULE