GSIC - Global Service Information Center

# FRONT DOOR BELT MOULDING > INSTALLATION

## for Preparation Click here

1. INSTALL FRONT DOOR BELT MOULDING ASSEMBLY LH

1. Put protective tape to the upper part of the door.

1. Attach the claws to install the moulding.

   HINT:
     Confirm that the moulding is firmly installed.

2. INSTALL OUTER REAR VIEW MIRROR SUB-ASSEMBLY LH

3. INSTALL FRONT DOOR TRIM BOARD SUB-ASSEMBLY LH

4. INSTALL FRONT ARMREST BASE PANEL UPPER LH (w/ Power Window)

5. INSTALL DOOR PULL HANDLE

6. INSTALL FRONT DOOR LOWER FRAME BRACKET GARNISH LH

7. INSTALL FRONT DOOR WINDOW REGULATOR HANDLE ASSEMBLY (w/o Power Window)

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.