GSIC - Global Service Information Center

### FUEL SUPPLY PUMP > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER (for 4WD)

3. REMOVE NO. 2 ENGINE UNDER COVER (for 4WD)

4. LOOSEN FUEL TANK CAP ASSEMBLY

5. DRAIN FUEL

6. DRAIN ENGINE COOLANT

7. DRAIN AUTOMATIC TRANSMISSION FLUID (for Automatic Transmission)

8. REMOVE RADIATOR ASSEMBLY

9. REMOVE NO. 1 TIMING BELT COVER

10. REMOVE TIMING BELT

11. REMOVE FUEL SUPPLY PUMP