GSIC - Global Service Information Center

# REAR SPEED SENSOR > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT REAR SPEED SENSOR

1. Measure the resistance of the sensor.

   Standard resistance:

     Tester Connection | Specified Condition
     1 (RL-) - 2 (RL+) | 0.6 to 1.8 kΩ
     1 (RL-) - Body ground | 10 kΩ or higher
     2 (RL+) - Body ground | 10 kΩ or higher

   1. If the result is not as specified, replace the speed sensor.

   HINT:
     Check the speed sensor signal after the speed sensor replacement.