GSIC - Global Service Information Center

### REAR SEAT OUTER BELT ASSEMBLY > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE REAR SEAT CUSHION ASSEMBLY LH (for Extra Cab)

3. REMOVE REAR SEAT CUSHION ASSEMBLY RH (for Extra Cab)

4. REMOVE QUARTER INSIDE TRIM BOARD LH (for Extra Cab)

5. REMOVE REAR SEAT ASSEMBLY (for Double Cab)

6. REMOVE REAR DOOR SCUFF PLATE LH (for Double Cab)

7. REMOVE REAR DOOR OPENING TRIM LH (for Double Cab)

8. REMOVE QUARTER TRIM PANEL LOWER LH (for Double Cab)

9. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH