GSIC - Global Service Information Center

# 1TR-FE IGNITION > SERVICE DATA

Spark plug | Recommended spark plug | DENSO made: K20HR-U11
Standard electrode gap for used spark plug | 1.0 to 1.1 mm (0.039 to 0.043 in.)
Maximum electrode gap for used spark plug | 1.3 mm (0.051 in.).
Crankshaft position sensor | Resistance | Cold: 1,630 to 2,740 Ω Hot: 2,065to 3,225 Ω
Camshaft position sensor | Resistance | Cold: 835 to 1,400 Ω Hot: 1,060 to 1,645 Ω