GSIC - Global Service Information Center

### WINDSHIELD GLASS > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE INNER REAR VIEW MIRROR ASSEMBLY

3. REMOVE ROOF HEADLINING ASSEMBLY

4. REMOVE FRONT WIPER ARM HEAD CAP

5. REMOVE FRONT WIPER ARM AND BLADE ASSEMBLY LH

6. REMOVE FRONT WIPER ARM AND BLADE ASSEMBLY RH

7. REMOVE HOOD TO COWL TOP SEAL

8. REMOVE COWL TOP VENTILATOR LOUVER LH

9. REMOVE COWL TOP VENTILATOR LOUVER RH

10. REMOVE WINDSHIELD MOULDING OUTER UPPER

11. REMOVE WINDSHIELD GLASS

12. CLEAN WINDSHIELD GLASS

13. CLEAN VEHICLE BODY