GSIC - Global Service Information Center

# COMBINATION METER > INSTALLATION

## for Preparation Click here

1. INSTALL COMBINATION METER ASSEMBLY

NOTICE:

  There are 2 types of combination meters. One type has a 40 pin connector and 16 pin connector. The other type only has a 40 pin connector.

1. Connect all connectors.

1. Install the combination meter with the 3 screws <B>.

2. INSTALL INSTRUMENT CLUSTER FINISH PANEL

1. Attach the 2 claws to install the panel.

1. Install the clip.

3. INSTALL STEERING COLUMN COVER UPPER

1. Install the cover lower with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

4. INSTALL STEERING COLUMN COVER LOWER

1. Install the cover lower with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

5. INSTALL STEERING WHEEL ASSEMBLY

1. Align the matchmarks on the steering wheel and main shaft.

1. Install the steering set nut.

   Torque:
     50 N*m{ 510 kgf*cm , 37 ft.*lbf }

6. INSTALL STEERING PAD ASSEMBLY

1. Support the steering pad with one hand as shown in the illustration.

1. Connect the airbag connector.

   NOTICE:
     When handling the airbag connector, do not damage the airbag wire harness.

1. Connect the horn connector.

1. Install the steering pad after confirming that the circumference grooves of the screws are caught on the screw case.

1. Using a T30 "torx" socket, install the 2 screws.

   Torque:
     8.8 N*m{ 90 kgf*cm , 78 in.*lbf }

7. PLACE FRONT WHEELS FACING STRAIGHT AHEAD

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

10. CHECK SRS WARNING LIGHT

1. Check the SRS warning light (Click here).