GSIC - Global Service Information Center

# A750F AUTOMATIC TRANSMISSION > SERVICE DATA

Line pressure Engine idling | D position | 362 to 423 kPa (3.7 to 4.3 kgf*cm2, 53 to 61 psi)
R position | 484 to 565 kPa (4.9 to 5.8 kgf*cm2, 70 to 82 psi)
Line pressure AT stall (Throttle valve fully opened) | D position | 1,282 to 1,381 kPa (13.1 to 14.1 kgf*cm2, 186 to 200 psi)
Engine stall revolution | D and R positions | 2,400 +- 150 rpm
Time lag | N → D position | Less than 1.2 seconds
N → R position | Less than 1.5 seconds
Engine idle speed (A/C OFF) | N position | 700 +- 50 rpm
Drive plate runout | Max. | 0.20 mm (0.0079 in.)
Torque converter runout | Max. | 0.30 mm (0.0118 in.)
Torque converter clutch installation distance | More than 17.1 mm (0.673 in.)
Shift schedule
D position | -
(Throttle valve fully opened) | 1 → 2 | 50 to 61 km/h (31 to 38 mph)
2 → 3 | 97 to 106 km/h (60 to 66 mph)
3 → 4 | 140 to 154 km/h (87 to 96 mph)
4 → 5 | 179 to 189 km/h (111 to 117 mph)
5 → 4 | 171 to 182 km/h (106 to 113 mph)
4 → 3 | 125 to 134 km/h (78 to 83 mph)
3 → 2 | 83 to 89 km/h (52 to 55 mph)
2 → 1 | 39 to 44 km/h (24 to 27 mph)
(Throttle valve fully closed) | 4 → 5 | 46 to 5 km/h (29 to 32 mph)
5 → 4 | 27 to 33 km/h (17 to 21 mph)
4 position | -
(Throttle valve fully opened) | 1 → 2 | 50 to 61 km/h (31 to 38 mph)
2 → 3 | 97 to 106 km/h (60 to 66 mph)
3 → 4 | 140 to 154 km/h (87 to 96 mph)
5 → 4 | 191 to 202 km/h (119 to 126 mph)
4 → 3 | 125 to 134 km/h (78 to 83 mph)
3 → 2 | 83 to 89 km/h (52 to 55 mph)
2 → 1 | 39 to 44 km/h (24 to 27 mph)
3 position
(Throttle valve fully opened) | 1 → 2 | 50 to 61 km/h (31 to 38 mph)
2 → 3 | 97 to 106 km/h (60 to 66 mph)
4 → 3 | 133 to 143 km/h (83 to 88 mph)
3 → 2 | 83 to 89 km/h (52 to 55 mph)
2 → 1 | 39 to 44 km/h (24 to 27 mph)
2 position
(Throttle valve fully opened) | 1 → 2 | 50 to 61 km/h (31 to 38 mph)
3 → 2 | 88 to 98 km/h (55 to 61 mph)
2 → 1 | 39 to 44 km/h (24 to 27 mph)
1 position
(Throttle valve fully opened) | 2 → 1 | 42 to 48 km/h (26 to 30 mph)
Lock-up point Throttle valve opening 5%
D position 5th gear | Lock-up ON | 57 to 63 km/h (35 to 39 mph)
Lock-up OFF | 50 to 55 km/h (31 to 34 mph)
4 position 4th gear | Lock-up ON | 69 to 74 km/h (43 to 46 mph)
Lock-up OFF | 61 to 67 km/h (38 to 42 mph)