GSIC - Global Service Information Center

# REAR DOOR LOCK > ON-VEHICLE INSPECTION

1. INSPECT REAR DOOR LOCK ASSEMBLY LH (DOUBLE CAB)

1. Apply battery voltage to the door lock and check operation of the door lock motor.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → Terminal 4 Battery negative (-) → Terminal 1 | Lock
     Battery negative (+) → Terminal 1 Battery positive (-) → Terminal 4 | Unlock

   1. If the result is not as specified, replace the door lock assembly.

2. INSPECT REAR DOOR LOCK ASSEMBLY RH (DOUBLE CAB)

1. Apply battery voltage to the door lock and check operation of the door lock motor.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → Terminal 4 Battery negative (-) → Terminal 1 | Lock
     Battery negative (+) → Terminal 1 Battery positive (-) → Terminal 4 | Unlock

   1. If the result is not as specified, replace the door lock assembly.