GSIC - Global Service Information Center

# REAR BUMPER (for Flat Type) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE REAR BUMPER BAR

1. Disconnect the 2 license plate light connectors.

1. Detach the 4 clamps.

1. Remove the 4 bolts and bumper bar.

3. REMOVE REAR BUMPER ARM LH

1. Remove the 2 bolts and bumper arm.

4. REMOVE REAR BUMPER ARM RH

1. Remove the 2 bolts and bumper arm.