GSIC - Global Service Information Center

# REAR SPEAKER (for Double Cab) > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. INSTALL REAR NO. 1 SPEAKER ASSEMBLY

1. Install the speaker to the door.

1. Using an air riveter or hand riveter, install the speaker with 3 new rivets.

   NOTICE:

   1. Riveter Do not pry the rivet with the riveter, as this will cause damage to the riveter and mandrel.

   2. Confirm that the rivets are seated properly against the speaker.
      Do not tilt the riveter when installing the rivet to the speaker.
      Do not leave any space between the rivet head and speaker.

   3. Do not leave any space between the speaker and door. Firmly hold together the 2 items while installing the rivet.

1. Connect the connector.

2. INSTALL REAR DOOR TRIM BOARD SUB-ASSEMBLY LH

1. Attach the 5 claws to install the weatherstrip inner.

1. Attach the 9 clips to install the trim board.

1. Install the screw labeled B and clip labeled C.

3. INSTALL REAR DOOR ARMREST BASE PANEL UPPER LH

1. Attach the 2 claws to install the window regulator switch.

1. Connect the switch connector.

1. Attach the 2 clips and 2 claws to install the base panel together with the switch.

4. INSTALL REAR DOOR PULL HANDLE

1. Install the screw and pull handle.

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.