GSIC - Global Service Information Center

# QUARTER WINDOW GLASS > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.
3. A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. REMOVE FRONT SEAT ASSEMBLY (Bench Seat Type)

1. Remove front seat assembly (Click here).

2. REMOVE FRONT SEAT ASSEMBLY (Separate Seat Type)

1. Remove front seat assembly (Click here).

3. REMOVE FRONT DOOR SCUFF PLATE LH

1. Using a screwdriver, detach the 8 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 4 clips and remove the scuff plate.

4. REMOVE FRONT DOOR OPENING TRIM WEATHERSTRIP LH

1. Using a screwdriver, detach the 8 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 4 clips and remove the scuff plate.

5. REMOVE BACK PANEL GARNISH UPPER

1. Using a screwdriver, detach the 4 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

6. REMOVE REAR SEAT CUSHION ASSEMBLY LH

1. Pull the seat cushion lock hook's release lever in the direction of the arrow, and then disconnect the hook on the front of the seat cushion.

1. Detach the seat cushion's 2 rear hooks from the vehicle body.

1. Remove the seat cushion.

7. REMOVE REAR SEAT CUSHION ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.

8. REMOVE BACK PANEL GARNISH LOWER

1. Using a screwdriver, detach the 6 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

9. REMOVE REAR SEATBACK ASSEMBLY

1. Remove the 2 bolts.

1. Lift up the seatback in the direction indicated by the arrow in the illustration to detach the 2 hooks from the vehicle body. Then remove the seatback.

   NOTICE:
     Be careful not to damage the vehicle body.

10. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

1. Using a screwdriver, detach the 2 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bracket cover in the direction indicated by the arrow in the illustration.

11. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

12. REMOVE QUARTER INSIDE TRIM BOARD LH

1. Using a clip remover, detach the 7 clips.

1. Using a screwdriver, detach the 6 claws and remove the trim board.

   HINT:
     Tape the screwdriver tip before use.

1. Detach the claws and remove the trim pocket from the trim board.

13. REMOVE QUARTER PILLAR GARNISH LH

1. Using a clip remover, detach the 2 clips and remove the garnish.

14. REMOVE ROOF SIDE GARNISH INNER UPPER LH

1. Using a clip remover, detach the 3 clips and remove the garnish.

15. REMOVE QUARTER WINDOW ASSEMBLY LH

NOTICE:

1. When separating the glass from the vehicle, be careful not to damage the vehicle's paint or interior/exterior ornaments.
2. Procedures must be performed with 2 people, where the second person supports the glass.

1. Remove the 2 bolts.

1. Remove the 2 bolts.

1. Remove the glass as shown in the illustration.

1. Remove the screw, bush, retainer and lock.

1. Remove the 2 screws, 2 washers, 2 retainers, 2 bushes and 2 hinges.

1. Remove the weatherstrip LH.