GSIC - Global Service Information Center

# DRIVE BELT > INSTALLATION

## for Preparation Click here

1. INSTALL DRIVE BELT

1. While turning the belt tensioner counterclockwise, align its holes, and then insert a bar of 6 mm (0.24 in.) into the holes to fix the belt tensioner.

1. Install the V-ribbed belt.

1. While turning the belt tensioner counterclockwise, remove the bar.

1. If it is hard to install the V-ribbed belt, perform the following procedure.

   1. Put the V-ribbed belt on everything except the P/S pump as shown in the illustration.

   2. While releasing the belt tension by turning the belt tensioner counterclockwise, put the V-ribbed belt on the P/S pump.