GSIC - Global Service Information Center

# INPUT SHAFT > REMOVAL

## for Preparation Click here

HINT:

  COMPONENTS: Click here.

1. REMOVE NO. 2 SYNCHRONIZER RING

1. Remove synchronizer ring from the input shaft.

2. REMOVE INPUT SHAFT BEARING

1. Remove the bearing from the input shaft.

3. REMOVE FRONT BEARING SHAFT SNAP RING

1. Using a snap ring expander, remove the snap ring from the input shaft.

4. REMOVE INPUT SHAFT FRONT BEARING

1. Using SST and a press, press out the front bearing from the input shaft.

   SST
     09950-00020

5. REMOVE NO. 2 SYNCHRONIZER RING

1. Apply gear oil to the cone of the input shaft, and check that it does not turn in both direction while pushing the No. 2 synchronizer ring.
   If it can turn, replace the No. 1 synchronizer ring .

1. Push the No. 2 synchronizer ring to the cone of the input shaft. Measure the clearance between the No. 2 synchronizer ring and input shaft.

   Standard clearance:
     0.70 to 1.70 mm (0.0276 to 0.0669 in.)
   If the clearance is not as specified, replace the synchronizer ring No. 2 with a new one.