GSIC - Global Service Information Center

# REAR SEAT OUTER BELT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

1. Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf } for bolt A

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf } for bolt B

1. Install the bolt and close the cover as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Install the floor anchor with the bolt, as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Install the floor anchor with the bolt, as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

2. INSTALL QUARTER TRIM PANEL LOWER LH (for Double Cab)

1. Attach the 3 clips and claw to install the trim panel.

3. INSTALL REAR DOOR OPENING TRIM LH (for Double Cab)

4. INSTALL REAR DOOR SCUFF PLATE LH (for Double Cab)

1. Attach the 2 clips and 7 claws to install the scuff plate.

5. INSTALL REAR SEAT ASSEMBLY (for Extra Cab)

1. Attach the seat cushion's 2 rear hooks to the vehicle body.

1. Attach the seat cushion's front hook to the rear seat cushion lock hook. Then install the seat cushion.

1. Confirm that the seat cushion is firmly installed.

6. INSTALL QUARTER INSIDE TRIM BOARD LH (for Extra Cab)

1. Attach the claws and install the trim pocket to the trim board.

1. Attach the 7 clips and 6 claws to install the trim board.

7. INSTALL REAR SEAT CUSHION ASSEMBLY RH (for Extra Cab)

1. Attach the seat cushion's 2 rear hooks to the vehicle body.

1. Attach the seat cushion's front hook to the rear seat cushion lock hook. Then install the seat cushion.

1. Confirm that the seat cushion is firmly installed.

8. INSTALL REAR SEAT CUSHION ASSEMBLY LH (for Extra Cab)

HINT:

  Use the same procedures described for the LH side.

9. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

10. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.