GSIC - Global Service Information Center

# DECELERATION SENSOR (for 4WD) > INSTALLATION

## for Preparation Click here

1. INSTALL DECELERATION SENSOR

1. Install the sensor with the 2 nuts.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

1. Connect the sensor connector.

1. Install the sensor cover with the bolt.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

2. INSTALL FRONT SEAT ASSEMBLY

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.