GSIC - Global Service Information Center

### FUEL INJECTOR > REMOVAL

1. DISCHARGE FUEL SYSTEM PRESSURE

2. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

3. DRAIN ENGINE COOLANT

4. REMOVE V-BANK COVER

5. DISCONNECT NO. 2 VENTILATION HOSE

6. REMOVE AIR CLEANER ASSEMBLY

7. REMOVE INTAKE AIR SURGE TANK

8. DISCONNECT NO. 1 FUEL PIPE SUB-ASSEMBLY

9. DISCONNECT NO. 2 FUEL PIPE SUB-ASSEMBLY

10. REMOVE FUEL DELIVERY PIPE SUB-ASSEMBLY

11. REMOVE INJECTOR ASSEMBLY