GSIC - Global Service Information Center

# STARTER > INSTALLATION

## for Preparation Click here

1. INSTALL STARTER ASSEMBLY

1. A/T:
   Install the starter and ground cable with the 2 nuts and bolt.

1. M/T:
   Install the starter and ground cable with the nut and bolt.

   Torque:
     68 N*m{ 693 kgf*cm , 50 ft.*lbf }

1. Install the starter wire to terminal 30 with the nut.

   Torque:
     9.8 N*m{ 100 kgf*cm , 7 ft.*lbf }

1. Connect the starter connector.

1. A/T:
   Install the A/T oil dipstick with the 2 bolts.

1. M/T:
   Install the clutch release cylinder.

2. INSTALL FRONT FENDER SEAL

1. Install the seal with the 5 clips.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.