GSIC - Global Service Information Center

# 1KD-FTV FUEL > SERVICE DATA

Supply pump (suction control valve) | Resistance | at 20 °C (68 °F) | 1.9 to 2.3 Ω
Injector | Resistance | at 20 °C (68 °F) | 0.85 to 1.05 Ω
Common rail | Resistance | 1-2 | 16.4 kΩ or less
2-3 | 3 kΩ or less
Level warning switch | Specified condition | 1-2 (ON) | Below 1Ω
1-2 (OFF) | 10kΩ or higher
Fuel filter assembly (Warning switch) | Resistance | at 20 °C (68 °F) | Below 1Ω
Fuel temperature sensor | Resistance | at 20 °C (68 °F) | 2.32 to 2.59 kΩ
at 80 °C (176 °F) | 0.310 to 0.326 kΩ
Supply pump drive shaft pulley | Thrust clearance | 0.15 to 0.55 mm (0.0059 to 0.0217 in.)