GSIC - Global Service Information Center

### DTC 01-D6 No Master (AUDIO H/U)

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area

01-D6*

With ignition switch on ACC or ON, component in which this code is recorded was disconnected from system or master component.

1. Wire harness
2. Radio receiver assembly

HINT:

  *: This code may be recorded depending on the battery condition or engine start voltage even if no failure is detected.

## INSPECTION PROCEDURE

1.CHECK POWER SOURCE CIRCUIT (RADIO RECEIVER ASSEMBLY)

1. Please follow this pages (see page).

   HINT:
     If the power source circuit is operating normally, proceed to the next step.

NEXT |

2.CHECK FOR DTC

1. Delete the DTC.

1. Check for DTCs again.

   OK:
     No DTC is output.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

END