GSIC - Global Service Information Center

### FRONT SEAT OUTER BELT ASSEMBLY > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE FRONT SEAT ASSEMBLY (for Separate Seat Type)

3. REMOVE FRONT SEAT ASSEMBLY (for Bench Seat Type)

4. REMOVE QUARTER TRIM PANEL LOWER LH (for Single Cab)

5. REMOVE QUARTER INSIDE TRIM BOARD LH (for Extra Cab)

6. REMOVE CENTER PILLAR GARNISH LOWER LH (for Double Cab)

7. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

8. REMOVE FRONT SHOULDER BELT ANCHOR ADJUSTER ASSEMBLY (for Extra cab and Double cab)

9. REMOVE SHOULDER BELT ANCHORAGE PLATE COVER (for Extra Cab and Double Cab)