GSIC - Global Service Information Center

# MASS AIR FLOW METER > INSTALLATION

## for Preparation Click here

1. INSTALL MASS AIR FLOW METER

1. Install a new O-ring to the MAF meter.

1. Install the MAF meter with the 2 screws.

1. Connect the MAF meter connector.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.