GSIC - Global Service Information Center

# ECM > INSTALLATION

## for Preparation Click here

1. INSTALL NO. 2 ECM BRACKET

1. Install the bracket with the 2 screws.

   Torque:
     3.0 N*m{ 31 kgf*cm , 27 in.*lbf }

2. INSTALL NO. 1 ECM BRACKET

1. Install the bracket with the 2 screws.

   Torque:
     3.0 N*m{ 31 kgf*cm , 27 in.*lbf }

3. INSTALL ECM

1. Install the ECM with the bolt and 2 nuts.

   Torque:
     12.5 N*m{ 127 kgf*cm , 9 ft.*lbf }

1. Connect the 4 connectors.

4. INSTALL GLOVE COMPARTMENT DOOR ASSEMBLY

1. Attach the 2 hinges to install the door.

1. Push in the sides of the glove compartment door, as indicated by the arrows in the illustration. Then close the door to engage it to the 2 stoppers.

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.