GSIC - Global Service Information Center

# CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY

1. Disconnect the oil control valve connector.

1. Remove the bolt and oil control valve.

1. Remove the O-ring from the oil control valve.