GSIC - Global Service Information Center

# IGNITION SWITCH > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE STEERING COLUMN COVER LOWER

1. Remove the 3 screws and cover lower.

   HINT:
     Turn the steering wheel to the right and left as necessary to remove the 3 screws and cover lower.

3. DISCONNECT CONNECTOR

1. Disconnect the 9 connectors and wire harness clamps from the steering column.

4. REMOVE IGNITION OR STARTER SWITCH ASSEMBLY

1. Detach the 2 claws and remove the switch from the steering column bracket upper.