GSIC - Global Service Information Center

# AIR CONDITIONING AMPLIFIER > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE AIR CONDITIONING AMPLIFIER ASSEMBLY

1. Detach the clamp.

1. Disconnect the connector.

1. Remove the screw and A/C amplifier.