GSIC - Global Service Information Center

# REAR SHOCK ABSORBER (for 2WD) > INSTALLATION

## for Preparation Click here

1. INSTALL REAR SHOCK ABSORBER ASSEMBLY

1. Install the 2 washers to the axle housing.

1. Install 4 new bushes to the absorber.

1. Install the absorber (with the 4 bushes) to the U bolt seat and frame.

1. Install the 2 washers.

1. Temporarily tighten the 2 bolts.

2. INSTALL REAR WHEEL

1. Install the wheel.

   Torque:
     152 N*m{ 1,550 kgf*cm , 112 ft.*lbf } for steel wheel
     121 N*m{ 1,234 kgf*cm , 89 ft.*lbf } for aluminum wheel

3. STABILIZE SUSPENSION

1. Lower the vehicle.

1. Bounce the vehicle up and down several times to stabilize the suspension.

4. TIGHTEN REAR SHOCK ABSORBER BOLT

1. Tighten the 2 bolts.

   Torque:
     105 N*m{ 1,070 kgf*cm , 77 ft.*lbf }