GSIC - Global Service Information Center

# CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL CAMSHAFT TIMING OIL CONTROL VALVE (for Bank 1)

1. Apply a light coat of engine oil to a new O-ring of the oil control valve.

1. Install the oil control valve with the bolt.

   Torque:
     9.0 N*m{ 92 kgf*cm , 80 in.*lbf }

   NOTICE:
     Be careful that the O-ring is not cracked when installing the oil control valve.

1. Connect the camshaft timing oil control valve connector.

2. INSTALL CAMSHAFT TIMING OIL CONTROL VALVE (for Bank 2)

1. Apply a light coat of engine oil to a new O-ring of the oil control valve.

1. Install the oil control valve with the bolt.

   Torque:
     9.0 N*m{ 92 kgf*cm , 80 in.*lbf }

   NOTICE:
     Be careful that the O-ring is not cracked when installing the oil control valve.

1. Connect the oil control valve connector.

3. INSTALL THROTTLE BODY

1. Install a new gasket to the intake air surge tank.

1. Install the throttle motor connector.

   Torque:
     11 N*m{ 112 kgf*cm , 9 ft.*lbf }

4. INSTALL AIR CLEANER ASSEMBLY

Torque:
  8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

5. INSTALL NO. 2 VENTILATION HOSE

6. INSTALL V-BANK COVER

Torque:
  7.5 N*m{ 76 kgf*cm , 66 in.*lbf }

7. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

8. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal