GSIC - Global Service Information Center

### EXHAUST PIPE > INSTALLATION

1. INSTALL FRONT EXHAUST PIPE ASSEMBLY

2. INSTALL HEATED OXYGEN SENSOR (for Unleaded Gasoline Specification Vehicle)

3. INSTALL AIR FUEL RATIO SENSOR (for Unleaded Gasoline Specification Vehicle)

4. INSTALL CENTER EXHAUST PIPE ASSEMBLY

5. INSTALL TAILPIPE ASSEMBLY

6. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

7. PERFORM INITIALIZATION

8. CHECK FOR EXHAUST GAS LEAKS