GSIC - Global Service Information Center

### STEERING KNUCKLE (for 4WD) > REMOVAL

1. REMOVE FRONT WHEEL

2. REMOVE FRONT SPEED SENSOR LH

3. REMOVE FRONT DISC BRAKE CALIPER ASSEMBLY LH

4. REMOVE FRONT DISC

5. REMOVE FRONT AXLE HUB GREASE CAP

6. REMOVE FRONT AXLE HUB NUT

7. DISCONNECT FRONT STABILIZER LINK ASSEMBLY LH

8. DISCONNECT TIE ROD END SUB-ASSEMBLY LH

9. DISCONNECT FRONT SUSPENSION LOWER ARM ASSEMBLY WITH ATTACHMENT LH

10. DISCONNECT FRONT SUSPENSION UPPER ARM ASSEMBLY

11. REMOVE FRONT AXLE HUB DUST SEAL

12. REMOVE FRONT AXLE HUB ASSEMBLY